**LIST OF AVAILABLE INTERRUPTS:**

**INT 21H**

You can choose one of DOS interrupts by setting AH register with:

* 0H:
  + this interrupt will terminate your program,
* 1H:
  + this interrupt will launch command terminal,
* 2H:
  + this interrupt will display a char, which respond to number in DL register (ASCII code),
* 19H:
  + this interrupt will set AL register with ASCII code of current disk letter,